M(1) Eighth Edition M(1)

NAME

M, U - conveniently mount and unmount

SYNOPSISS

M device [- r] U device

OPTIONS

- r Mount read-only

EXAMPLES M root # Mount the RAM image on/root

M 0 # Mount /dev/fd0 on/fd0

U fd1 # Unmount /dev/fd1 from /fd1

DESCRIPPTION M and U allow easy mounting and unmounting of a device by using only an abbreviated device name or keyword. Special keywords are root, tmp , and usr for the three hard disk partitions Minix runs in. Floppy devices are mounted on /fd0 or /fd1. You can use 0 and 1 instead of fd0 and fd1. A device it doesn’t know about is mounted on /mnt.

SEE AALSO

mount (1), umount (1).

Page 1 May 7, 2001