RECWAVE (1) Eighth Edition RECWAVE (1)

NAME

recwave - record an audio file in MicroSoft PCM wave format SYNOPSISS

recwave [- b -s - r] file DESCRIPPTION Recwav takes samples from /dev/audio and writes them to file in Microsoft PCMwave format.

OPTIONS

- b number of bits to use for one sample. Must be 8 or 16, default is 8 - s enable stereo sampling. 0 = mono (default), 1 = stereo - r sample rate in samples/sec. 4000 - 44100 (default 22050) BUGS

The highest sample rate that can be used depends on the speed of the system and the size of the DMA buffer used in the driver. (/usr/src/kernel/sb16.h) AUTHOR

Michel R. Prevenier (mrpreve@cs.vu.nl)

Page 1 May 7, 2001