LOADFONT( 1) Eighth Edition LOADFONT (1)

NAME

loadfont - load a font into the video card

SYNOPSISS

loadfont fontfile

EXAMPLES loadfont iso1.fnt # Loads theISO 8859-1 (Latin-1) font

DESCRIPPTION Loadfont loads a custom font into the video card (EGA or VGA). The font character size has to be 8x16 pixels and the font file must contain 256 characters for a total size of 4 kilobytes.

Loadfont together with loadkeys allow the console and keyboard to be customized to national conventions.

If it exists, the file /etc/fontis loaded asa custom font by/usr/etc/rc at boot time.

SEE AALSO

console(4).

Page 1 May 7, 2001