STTY(1) Eighth Edition STTY(1)

NAME

stty - set terminal parameters

SYNOPSISS

stty [- ag]

stty encoded-form

stty speed ispeed speed ospeed speed cs5 cs6 cs7 cs8 [- ]parenb [- ]parodd [-]hupcl [- ]cstopb [- ]cread [- ]clocal [- ]ignbrk [- ]brkint [- ]ignpar [-]parmrk [- ]inpck [- ]istrip [-]inlcr [- ]igncr [-]icrnl [- ]ixon [- ]ixoff [-]ixany [- ]opost [-]onlcr [- ]xtabs [- ]onoeot [- ]isig [- ]icanon [-]iexten [- ]echo [-]echoe [- ]echok [- ]echonl [- ]noflsh [- ]lflusho eof=c eol=c erase=c erase =c intr =c kill=c quit=c susp=c start =c stop=c rprnt =c lnext=c flush=c min=n time=n rows n cols n xpixels n ypixels n cooked raw [- ]evenp [-]parity [- ]oddp [- ]nl ek sane

DESCRIPPTION Stty shows or changes the parameters of the terminal connected to standard input. Stty takes a myriad of arguments most of which are mapped directly to the flags and special characters described in tty(4), so we won’t describe them here.

Stty has three forms of operation. First, without any arguments stty shows all terminal attributes that are different from the default state. Option - a makes stty print all terminal attributes, and - g lets stty print the attributes in a special encoded form, a simple row of colon separated hexadecimal numbers.

In the second form of operation stty takes an encoded form as produced by the -g option and sets the terminals attributes to its decoded value.

In the third form stty interprets a series of flags and parameters settings and modifies the terminal attributes accordingly. Flags can be given as icanon or - icanon for instance, either setting or clearing the ICANON flag. Special character values can by set like intr=^C for example, which sets the interrupt character to CTRL-C. You can either use a real CTRL-C, or the two characters ‘^’ and ‘C’. In any case it is probably necessary to use quotes to guard it from the shell: intr=’^C’ .

A number alone is interpreted as a baud rate setting for both the input and output rate. The input or the output rate can be set separately with use of theispeed and ospeed prefixes to the number. The character size can be set with cs5, cs6, cs7 or cs8.

The MIN and TIME value, the number of rows and columns, and the xpixels and ypixels of the window can also be set using one of the keywords min, time, rows, cols, xpixels or ypixels, followed by a decimal number that is the value of the setting.

Stty accepts several keywords that are not named by corresponding flags or parameters in tty(4). They set several attributes at once:

cooked Same as icrnl ixon opost onlcr isig icanon iexten echo, setting all the attributes that are needed for line oriented mode.

raw Same as -icrnl - ixon - opost - onlcr - isig -icanon - iexten - echo, setting all the attributes for a raw data channel.

evenp parity

These synonyms are equal to cs7 parenb - parodd , setting theline to 7 bits even parity.

oddp Same as cs7 parenb parodd , setting theline to 7 bits oddparity.

- parity - evenp - oddp

All synonyms for cs8 -parenb , setting theline to 8 bits, no parity.

nl Same as icrnl, setting carriage return to line feed input translation.

- nl Same as - icrnl - inlcr -igncr , disabling any carriage return or linefeed handling.

ek Set the ERASE and KILL special characters back to the default.

sane Set all attributes to the default exceptthings like the linespeed and parity, because their "sane" value is probably what it is right now. The default values are compiled into stty from the

Page 1 May 7, 2001

STTY(1) Eighth Edition STTY(1)

<termios.h> include file. Use stty sane; stty -a to know what they are.

FILLES

/etc/ttytab The init field of this file may contain an stty command to set the attributes to match an attached RS232 terminal or modem.

SEE AALSO tty(4), ttytab (5).

NOTES

The cooked, raw , rows, cols, xpixels and ypixels keywords are Minix additions beyond the keywords defined by POSIX. Rows and cols are common UNIX extensions, however. There are more Minix specific flags that match the Minix specific attributes described in tty(4).

AUTHOR Kees J. Bot (kjb@cs.vu.nl)

May 7, 2001 Page 2